Oziexplorer:

Find GPS com port (can use program: “GPSInfo” or look thru com ports of computer)

File -> Configuration (crtl c):

Com tab: General COM settings – chose GPS port

Moving Map->Start NMEA Communication with GPS

 Should get location showing on map (red arrow)

Navigation ->Navigation Control (ctrl N) to get waypoints and route options

Moving Map Control -> Start/Stop NMEA, keep map center, etc. options

Load->Load waypoints from file-> chose waypoints

 Use button next to “Next Wp” to select next station on route. No active routes, as these change trip to trip.

Tracks: Make sure Configuration-> Track tab has “Track Log File” set to ‘Daily’

 Under “Moving Map”, make sure you have selected:

 ‘Log track tail’ and ‘Log track to file’

View-> ‘Show tracks on Map’ and select “Track Control” to save/export/edit tracks.

 Tracks usually get saved in the c:\Oxiexplorer\Data folder – search by file date.

For Neocaligus to import to their program Nobeltek, need .onf file for waypoints? Doesn’t take ozi exported files (.txt, .csv, .wpx)?