








Cruise Number: _2024-008____
[osdcommon\cruise_data_processing\2024-008\ARCHIVE]
[osdcommon\cruise_data_processing\2024-008\ARCHIVE\Bottle] *.CHE
[osdcommon\cruise_data_processing\2024-008\ARCHIVE\CTD] *.CTD
[osdcommon\cruise_data_processing\2024-008\ARCHIVE\DOC] general documents 
[osdcommon\cruise_data_processing\2024-008\ARCHIVE\DOC\Hydro] documents re CHE files
[osdcommon\cruise_data_processing\2024-008\ARCHIVE\DOC\TSG] documents re TSG files

[osdcommon\cruise_data_processing\2024-008\ARCHIVE\DOC\TSG] documents re TSG files

[osdcommon\cruise_data_processing\2024-008\ARCHIVE\DOC\LOOP] documents re LOOP file

[osdcommon\cruise_data_processing\2024-008\ARCHIVE\LOGS] 
[osdcommon\cruise_data_processing\2024-008\ARCHIVE\UNDERWAY\TSG] *.tob -TSG data
[osdcommon\cruise_data_processing\2024-008\ARCHIVE\UNDERWAY\Loop] *.loop
[osdcommon\cruise_data_processing\2024-008\PROCESSING\CTD] 

[osdcommon\cruise_data_processing\2024-008\PROCESSING\CTD\CONVERT] *.CNV – after conversion

[osdcommon\cruise_data_processing\2024-008\PROCESSING\CTD\DERIVE] 

*.CNV – after conversion, wfilter, align, celltm, derive
[osdcommon\cruise_data_processing\2024-008\PROCESSING\CTD\IOS] 

*.avg - data after metre-averaging using BINAVE (downcast)


*.cln - after adding event #s and removing pad values from pressure


*.cor1 and *.cor2 - after recalibration


*.ctd - final files 


*.del – after DELETE


*.edt & *.log– after graphical editing 


*.ios - data after conversion to IOS HEADERS

*.rem – after REMOVE 

*.reo – 2nd last step - after addition of DO in mass units and reorder

[osdcommon\cruise_data_processing\2024-008\PROCESSING\DOC] 

2024-008_Processing_Report.doc - processing notes
2024-008_File.doc - this document
2024-008-ctd_final.rpt – CTD file header check including channel summary
2024-008-ctd_xref.txt – cross-reference list of casts

2024-008-recal-CTD.ccf – recal file for DO, salinity
2024-008-recal-CTD2.ccf – recal file for DO, salinity


2024-008-recal-SIL.ccf - recal file for Silicate (if Sal<25)


2024-008-altimeter.csv – water depth check

2024-008-hdr-CTD1.txt – Header comments

[osdcommon\cruise_data_processing\2024-008\PROCESSING\DOC\Hydro]

2024-008_CHL.csv – extracted chlorophyll data simplified from analyst’s s/s

2024-008_NUTS.csv – nutrients simplified from analyst’s s/s
2024-008_OXY.csv – dissolved oxygen data simplified from analyst’s s/s

2024-008_SAL.csv – salinity data from Autosal, simplified from analyst’s s/s

2024-008_DMS.csv – DMS data simplified from analyst’s s/s

2024-008_DMSP.csv – DMSP data simplified from analyst’s s/s

2024-008-che-final.rpt – final header check of CHE files

2024-008_hydro_xref.txt – cross-reference listing of bottle files (BOT and CHE)
2024-008-bot-hdr.txt – header file with comments for BOT files
Addsamp.csv – spreadsheet relating bottle numbers to sample numbers

2024-008-oxy-comp1.xls – comparison of titrated DO & CTD DO

2024-008-oxy-comp2.xls – comparison of titrated DO & CTD DO

2024-008-oxy-comp3.xls – comparison of titrated DO & CTD DO
2024-008-sal-comp1.csv – comparison of rosette bottle and CTD salinity 

2024-008-sal-comp2.csv – comparison of rosette bottle and CTD salinity 

[osdcommon\cruise_data_processing\2024-008\PROCESSING\DOC\TSG]

2024-008-CTDvsTSG.xlsx – comparison of Loops, CTD and TSG

2024-008-hdr-tsg.txt – header file with comments for TOB files

2024-008-TSG-xref.txt -- cross-reference list of samples

[osdcommon\cruise_data_processing\2024-008\PROCESSING\DOC\Loop]


2024-008-loop-hdr.txt – header file with comments for loop file

[osdcommon\cruise_data_processing\2024-008\PROCESSING\hydro] 
*.cheprelim – files after merging in chemistry

*.che – Final files for SBE911
*.mrgcor1 and .mrgcor2 – after recalibration of silicate and DO, Sal
*.mrgcorsil – after correction of silicate where sal<25

*.mrgrem – after removing unnecessary channels from SBE911

*.mrgreo – 2nd last step after reorder

*.ros – after initial conversion from SBE911
[osdcommon\cruise_data\2024-008\PROCESSING\TSG]

*.atc – addition of Time & Date channels calculated from Julian Time

*.cln – after adding positions and times to headers and time/date channels

*.der – after derivation of sigma-T

*.edt & *flag – after editing

*.ios – after conversion to IOS HEADERS

*.rem – after removing flag and scan #


*.tob – final files

[osdcommon\cruise_data\2024-008\PROCESSING\Loop]


2024-008-surface_data.csv – data pulled together


2024-008-surface.loop – loop file

