File List for SeaBird Data          Cruise Number: _2025-001
[osdcommon\cruise_data\2025-001\ARCHIVE]

[osdcommon\cruise_data\2025-001\ARCHIVE\Bottle] *.CHE

[osdcommon\cruise_data\2025-001\ARCHIVE\CTD] *.CTD 
[osdcommon\cruise_data\2025-001\ARCHIVE\DOC] most documents from RAW and PROCESSING

[osdcommon\cruise_data\2025-001\ARCHIVE\DOC\HYDRO] COMPARE files 
[osdcommon\cruise_data\2025-001\ARCHIVE\DOC\TSG] TSG documents
[osdcommon\cruise_data\2025-001\ARCHIVE\DOC\Loop] Loop spreadsheet
[osdcommon\cruise_data\2025-001\ARCHIVE\LOGS] any scanned or S/S logs
[osdcommon\cruise_data\2025-001\ARCHIVE\Underway] TSG and Loop data
[osdcommon\cruise_data\2025-001\PROCESSING]  

[osdcommon\cruise_data\2025-001\PROCESSING\CONVERT]
*.CNV – after conversion

[osdcommon\cruise_data\2025-001\PROCESSING\DERIVE]*.CNV – after convert/wildedit/celltm/derive
[osdcommon\cruise_data\2025-001\PROCESSING\DOC] 


2025-001-recal1.ccf – calibration control file
2025-001_File.doc - this document

2025-001_Processing_Report.doc - processing notes
2025-001-ctd.xmlcon – configuration files used in processing
2025-001-ctd-final.rpt – CTD file header check including channel summary
2025-001-ctd-xref.txt – cross reference list of CTD files

2025-001-altimeter-ctd.xls – reports on header entries for altimetry before & after fixing water depths
Cond_SBE4_****.xml – post-cruise conductivity calibrations

*hdr.txt – header file with comments for CTD files
[osdcommon\cruise_data\2025-001\PROCESSING\DOC\hydro] 


2025-001-chl-fl-comp1csv&..xls – comparison of extracted CHL and CTD Fluorometer
2025-001-dox-comp1.csv & .xls – initial comparison of titrated DO & CTD DO
2025-001-dox-comp1a.xls – comparison using updated factor E

2025-001-dox-comp2.csv &.xls –comparison of titrated DO & CTD DO after initial recal
2025-001-dox-comp3.csv &xls – comparison of titrated DO & downcast CTD DO
2025-001-sal-comp1.csv & xls –initial comparison of rosette bottle and CTD salinity 
2025-001-sal-comp2.csv & xls –initial comparison of rosette bottle and CTD salinity 

Addsamp_new.csv – spreadsheet relating bottle numbers to sample numbers
2025-001-bottles.xslx – summary of bottle data in CHE files 
2025-001-che-final.rpt – final header check of bottle files 

2025-001-che-xref.txt – cross-reference listing of bottle files
2025-001 hydro.xlsx – doc from Chief Scientist with CTD data plus initial titrated DO data and plots
*hdr.txt – header files with comments for CHE files – 2 groups
[osdcommon\cruise_data\2025-001\PROCESSING\DOC\hydro\hysteresis tests] tests for SBE Oxygen

[osdcommon\cruise_data\2025-001\PROCESSING\DOC\hydro\Python_input] to create CHEPRELIM

[osdcommon\cruise_data\2025-001\PROCESSING\DOC\hydro\python_output] output of python routine
[osdcommon\cruise_data\2025-001\PROCESSING\DOC\Loop]

 2025-001-loop-hdr.txt – header comments for loop file


 2025-001-loops.xls – information provided by chief scientist
[osdcommon\cruise_data\2025-001\PROCESSING\DOC\tsg] 
2025-001-tsg-ctd-loop-rosette-comp.xlsx – comparisons of TSG data, loop, CTD, rosette
2025-001-surface.csv – surface data from rosette files

2025-001-hdr-tsg.txt – header with comments for TOB files.

2025-001-tsg.xmlcon – calibration control file for TSG

[osdcommon\cruise_data\2025-001\PROCESSING\HYDRO]


*.bot - ros files converted to IOS HEADERS + added event numbers – used only for COMPARE
*.che – final bottle-averaged rosette files merged with chemistry data
*.cheprelim – initial output of python routine (missing PAR)
*.cheprelim2 – after merge of cheprelim & iosPAR

2025-001-0070.cheprelima & 2025-001-0070.cheprelimb – files from split cast 70
*.ed1 & *.log – output of CTDEDIT for Event 14
*.iosP & iosPS - converted files with PAR before and after SORT

*.iosPAR – after files *.iosPS put through CLEAN to remove excess headers
*.mrgcor1 – after correction of dissolved oxygen, pressure, depth, salinity
*.mrgox1 & mrgox2 – after correction of DO volume + mass units

*.mrgrem – after removal of unneeded channels

*.mrgreo – just before final step running Head Edit
*.mrgsort – after calibration and reordering on pressure
*.ros  - rosette files created by DATCNV, no other processing done.



*.sam – bottle files with CTD data & sample numbers added.
*.samcor1 – after recalibration of SAM files

*.thn – bin-averaged & thinned downcast files for comparison with upcast bottles

Hydro.txt – list of rosette casts

[osdcommon\cruise_data\2025-001\PROCESSING\IOS] after conversion to IOS SHELL
*.avg - data after metre-averaging using BINAVE 


*.cln - data after conversion to IOS HEADERS and a run of CLEAN
*.cor1 –after recalibration of SBE DO


*.ctd - final files 

*.del & *.delpred– after DELETE – 2nd has output of AI predictive model – files used in CTDEDT
*.edt & *.log - output of CTDEDIT (an EDT file is prepared even if no editing is required.)

*.ios – data after conversion to IOS SHELL format 


*.rem – after removing some channels


*.reo – files just before header edit

Delete.log - log from routine DELETE 
[osdcommon\cruise_data\2025-001\PROCESSING\Loop] before conversion to IOS SHELL

2025-001-surface.loop – final loop file

2025-001-surface-6linehdr.csv – surface data from CHE and loop sample data with 6-line headers

2025-001-0001.iosloop –6linehdr csv file converted to IOS Header format

2025-001-0001.clnloop – as above with start and end times added 

 [osdcommon\cruise_data\2025-001\PROCESSING\TSG] before conversion to IOS SHELL

*.atc – after addition of record # and Julian time

*.avg – data averaged over 1 minute for comparison to CTD
*.cln – after adding positions and times to headers and time/date channels

*.cnv – after initial conversion
*.dsp – after running simple despike routine on salinity
*.ed1 & .log– after removing temp, sal, cond and fluor from initial 90 minutes
*.ios – after conversion to IOS HEADERS

*.rem – after removing fluorescence, pressure, T difference and record #

*.reo –TSG files after REORDER

*.tob – final file
2025-001-dsp.csv – s/s with *.dsp data

2025-001-0001-avg.csv – binned *.dsp data for use in comparison to CTD data
