File List for SeaBird Data          Cruise Number: _2025-005
[osdcommon\cruise_data\2025-005\ARCHIVE]

[osdcommon\cruise_data\2025-005\ARCHIVE\Bottle] *.CHE

[osdcommon\cruise_data\2025-005\ARCHIVE\CTD] *.CTD 
[osdcommon\cruise_data\2025-005\ARCHIVE\DOC] most documents from RAW and PROCESSING

[osdcommon\cruise_data\2025-005\ARCHIVE\DOC\HYDRO] COMPARE files 
[osdcommon\cruise_data\2025-005\ARCHIVE\LOGS] any scanned or S/S logs
[osdcommon\cruise_data\2025-005\PROCESSING]  

[osdcommon\cruise_data\2025-005\PROCESSING\CONVERT]
*.CNV – after conversion

[osdcommon\cruise_data\2025-005\PROCESSING\DERIVE]*.CNV – after convert/wildedit/celltm/derive
[osdcommon\cruise_data\2025-005\PROCESSING\DOC] 


2025-005-recal1.ccf – calibration control file
2025-005-recal-SIL.ccf - calibration control file for Bottle files only

2025-005_File.doc - this document

2025-005_Processing_Report.doc - processing notes
2025-005-ctd.xmlcon – configuration files used in processing
2025-005-ctd-final.rpt – CTD file header check including channel summary
2025-005-ctd-xref.txt – cross reference list of CTD files

2025-005-altimeter-ctd.xls – reports on header entries for altimetry before & after fixing water depths

*hdr.txt – header file with comments for CTD files
[osdcommon\cruise_data\2025-005\PROCESSING\DOC\hydro] 


2025-005-chl-fl-comp1csv&..xls – comparison of extracted CHL and CTD Fluorometer
2025-005-dox-comp1.csv & .xls – initial comparison of titrated DO & CTD DO
2025-005-dox-comp2.csv &.xls –comparison of titrated DO & CTD DO after initial recal
2025-005-dox-comp3.csv &xls – comparison of titrated DO & downcast CTD DO
2025-005-sal-comp1.csv & xls –initial comparison of rosette bottle and CTD salinity  

Addsamp.csv – spreadsheet relating bottle numbers to sample numbers
2025-005-bottles.xslx – summary of bottle data in CHE files 
2025-005-che-final.rpt – final header check of bottle files 

2025-005-che-xref.txt – cross-reference listing of bottle files
2025-005CHL.csv -summary of CHL sample data for bottle files

2025-005nuts.csv -summary of nutrient sample data for bottle files

2025-005sal.csv -summary of salinity sample data for bottle files

2025-005oxy.csv -summary of dissolved oxygen sample data for bottle files

*hdr.txt – header file with comments for CHE files
[osdcommon\cruise_data\2025-005\PROCESSING\HYDRO]


*.bot - ros files converted to IOS HEADERS + added event numbers – used only for COMPARE
*.che – final bottle-averaged rosette files merged with chemistry data
*.cheprelim – output of python routine 
2025-005-0050.cheprelima & 2025-005-0050.cheprelimb – files from split cast 50
*.cheprelimcor1 – after correction of dissolved oxygen and secondary salinity

*.cheprelimcorsil – after correction of silicate where salinity <25

*.cln – Step after *.ios to add event #s
*.ed1 & *.log – output of CTDEDIT for Event 14
*.ios – data converted to IOS Header

*.mrgcor1 – after correction of dissolved oxygen, pressure, depth, salinity
*.mrgox1 & mrgox2 – after correction of DO volume + mass units

*.mrgrem – after removal of unneeded channels

*.mrgreo – just before final step running Head Edit
*.mrgsort – after calibration and reordering on pressure
*.ros  - rosette files created by DATCNV, no other processing done.



*.sam & samavg – bottle files with CTD data & sample numbers added.
*.samcor1 – after recalibration of SAM files

*.thn – bin-averaged & thinned downcast files for comparison with upcast bottles

Hydro.txt – list of rosette casts

[osdcommon\cruise_data\2025-005\PROCESSING\IOS] after conversion to IOS SHELL
*.avg - data after metre-averaging using BINAVE 

*.clip1 – data removed from a few files (1,3,4,78)

*.clip – all files at CLIP stage whether clipped or not


*.cln - data after conversion to IOS HEADERS and a run of CLEAN
*.cor1 –after recalibration of SBE DO


*.ctd - final files 

*.del & *.delpred– after DELETE – 2nd has output of AI predictive model – files used in CTDEDT
*.edt & *.log - output of CTDEDIT (an EDT file is prepared even if no editing is required.)

*.ios – data after conversion to IOS SHELL format 


*.rem – after removing some channels


*.reo – files just before header edit

*.unt – after addition of DO in mass units

Delete.log - log from routine DELETE 
