Mooring Deployment Record

|  |  |
| --- | --- |
| Project Name:WCTSS | Scientific Authority: Charles Hannah |
| Project Area: Vancouver Harbour |
| Mooring Name: BUW02-B | Station Name:BUW02 |
| Latitude: 49° 17.669’ N | Longitude: 123° 1.926’ W |
| Depth: 45 | Tide: |
| Date: 20/12/2016 | Time: 1831 |
| Time Zone: UTC | Hovercraft deployment |
| Remarks: ADCP in stainless steel frame with 8 ViniesSBE37 attached to stainless frame |

Recovery

|  |  |
| --- | --- |
| Date: 14/6/2017 | Time: 1904 |
| Remarks:The mooring appeared to have shifted Southwest from its original location |

Instruments

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Type | Serial # | Depth | Time In | Time Out | Notes |
| WH600 | 3694 | 42 |  |  |  |
| SBE37 | 9652 | 43 |  |  | Mounted on ADCP frame |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

Releases

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Release | Serial # | Enable  | Release | Other |
| AR861 | 740 | 16BA | 1655 | 1649-Diagnostic |
|  |  |  |  |  |

Pingers

|  |  |  |  |
| --- | --- | --- | --- |
| Pinger | Serial # | Voltage | Frequency |
|  |  |  |  |
|  |  |  |  |

Flotation

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Type  | Serial # | Size | Colour | Type  | Serial # | Size | Colour |
| Vinyx8 |  | 13 | Orange |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |